# Overhauled summer 2015 by Dr. Azzy (Spence Konde) and again in early 2016 to add support for more chips. 

menu.chip=Chip
menu.clock=Clock
menu.bod=B.O.D.
menu.vcc=Voltage
menu.pinmapping=Pin Mapping
menu.INITIALIZE_SECONDARY_TIMERS=Initialize Secondary Timers
menu.TimerClockSource=Timer 1 Clock
menu.LTO=LTO (1.6.11+ only)






attinyx4.name=ATtiny24/44/84
attinyx4.upload.maximum_size=8192
attinyx4.upload.maximum_data_size=512
attinyx4.upload.tool=avrdude
attinyx4.build.board=AVR_ATTINYX4
attinyx4.bootloader.tool=avrdude
attinyx4.bootloader.unlock_bits=0xFF
attinyx4.bootloader.lock_bits=0xFF
attinyx4.menu.LTO.disable=Disabled
attinyx4.menu.LTO.disable.ltocflags=
attinyx4.menu.LTO.disable.ltoelfflags=
attinyx4.menu.LTO.disable.ltocppflags=
attinyx4.menu.LTO.disable.ltoarcmd=
attinyx4.menu.LTO.enable=Enabled
attinyx4.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx4.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx4.menu.LTO.enable.ltocppflags=-flto
attinyx4.menu.LTO.enable.ltoarcmd=gcc-
attinyx4.menu.chip.84=ATtiny84
attinyx4.menu.chip.84.build.mcu=attiny84
attinyx4.menu.chip.84.upload.maximum_size=8192
attinyx4.menu.chip.84.upload.maximum_data_size=512
attinyx4.menu.chip.44=ATtiny44
attinyx4.menu.chip.44.build.mcu=attiny44
attinyx4.menu.chip.44.upload.maximum_size=4096
attinyx4.menu.chip.44.upload.maximum_data_size=256
attinyx4.menu.chip.24=ATtiny24
attinyx4.menu.chip.24.build.mcu=attiny24
attinyx4.menu.chip.24.upload.maximum_size=2048
attinyx4.menu.chip.24.upload.maximum_data_size=128
attinyx4.build.core=tiny
attinyx4.bootloader.extended_fuses=0xFF
attinyx4.menu.clock.8internal=8 MHz (internal)
attinyx4.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx4.menu.clock.8internal.build.f_cpu=8000000L
attinyx4.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.20external=20 MHz (external)
attinyx4.menu.clock.20external.bootloader.low_fuses=0xFF
attinyx4.menu.clock.20external.build.f_cpu=20000000L
attinyx4.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.16external=16 MHz (external)
attinyx4.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx4.menu.clock.16external.build.f_cpu=16000000L
attinyx4.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.12external=12 MHz (external)
attinyx4.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx4.menu.clock.12external.build.f_cpu=12000000L
attinyx4.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.8external=8 MHz (external)
attinyx4.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx4.menu.clock.8external.build.f_cpu=8000000L
attinyx4.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.6external=6 MHz (external)
attinyx4.menu.clock.6external.bootloader.low_fuses=0xFD
attinyx4.menu.clock.6external.build.f_cpu=6000000L
attinyx4.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.4external=4 MHz (external)
attinyx4.menu.clock.4external.bootloader.low_fuses=0xFD
attinyx4.menu.clock.4external.build.f_cpu=4000000L
attinyx4.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx4.menu.clock.1internal=1 MHz (internal)
attinyx4.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx4.menu.clock.1internal.build.f_cpu=1000000L
attinyx4.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx4.menu.bod.disable=B.O.D. Disabled
attinyx4.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx4.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx4.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx4.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx4.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx4.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx4.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx4.menu.pinmapping.old=Counterclockwise (like ATTinyCore)
attinyx4.menu.pinmapping.old.build.variant=tinyX4
attinyx4.menu.pinmapping.new=Clockwise (like damellis core)
attinyx4.menu.pinmapping.new.build.variant=tinyX4_reverse


attinyx5.name=ATtiny25/45/85
attinyx5.upload.maximum_size=8192
attinyx5.upload.maximum_data_size=512
attinyx5.upload.tool=avrdude
attinyx5.bootloader.tool=avrdude
attinyx5.bootloader.unlock_bits=0xFF
attinyx5.bootloader.lock_bits=0xFF
attinyx5.build.core=tiny
attinyx5.build.board=AVR_ATTINYX5
attinyx5.bootloader.extended_fuses=0xFF
attinyx5.menu.LTO.disable=Disabled
attinyx5.menu.LTO.disable.ltocflags=
attinyx5.menu.LTO.disable.ltoelfflags=
attinyx5.menu.LTO.disable.ltocppflags=
attinyx5.menu.LTO.disable.ltoarcmd=
attinyx5.menu.LTO.enable=Enabled
attinyx5.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx5.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx5.menu.LTO.enable.ltocppflags=-flto
attinyx5.menu.LTO.enable.ltoarcmd=gcc-
attinyx5.menu.TimerClockSource.default=CPU
attinyx5.menu.TimerClockSource.pll=64MHz
attinyx5.menu.TimerClockSource.pll.build.extra_flags=-DPLLTIMER1
attinyx5.menu.TimerClockSource.lowpll=32MHz
attinyx5.menu.TimerClockSource.lowpll.build.extra_flags=-DLOWPLLTIMER1
attinyx5.menu.chip.85=ATtiny85
attinyx5.menu.chip.85.build.mcu=attiny85
attinyx5.menu.chip.85.upload.maximum_size=8192
attinyx5.menu.chip.85.upload.maximum_data_size=512
attinyx5.menu.chip.45=ATtiny45
attinyx5.menu.chip.45.build.mcu=attiny45
attinyx5.menu.chip.45.upload.maximum_size=4096
attinyx5.menu.chip.45.upload.maximum_data_size=256
attinyx5.menu.chip.25=ATtiny25
attinyx5.menu.chip.25.build.mcu=attiny25
attinyx5.menu.chip.25.upload.maximum_size=2048
attinyx5.menu.chip.25.upload.maximum_data_size=128
attinyx5.menu.clock.8internal=8 MHz (internal)
attinyx5.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx5.menu.clock.8internal.build.f_cpu=8000000L
attinyx5.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.16pll=16 MHz (PLL)
attinyx5.menu.clock.16pll.bootloader.low_fuses=0xF1
attinyx5.menu.clock.16pll.build.f_cpu=16000000L
attinyx5.menu.clock.16pll.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.20external=20 MHz (external)
attinyx5.menu.clock.20external.bootloader.low_fuses=0xFF
attinyx5.menu.clock.20external.build.f_cpu=20000000L
attinyx5.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.16external=16 MHz (external)
attinyx5.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx5.menu.clock.16external.build.f_cpu=16000000L
attinyx5.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.12external=12 MHz (external)
attinyx5.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx5.menu.clock.12external.build.f_cpu=12000000L
attinyx5.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.8external=8 MHz (external)
attinyx5.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx5.menu.clock.8external.build.f_cpu=8000000L
attinyx5.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.6external=6 MHz (external)
attinyx5.menu.clock.6external.bootloader.low_fuses=0xFD
attinyx5.menu.clock.6external.build.f_cpu=6000000L
attinyx5.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.4external=4 MHz (external)
attinyx5.menu.clock.4external.bootloader.low_fuses=0xFD
attinyx5.menu.clock.4external.build.f_cpu=4000000L
attinyx5.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.1internal=1 MHz (internal)
attinyx5.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx5.menu.clock.1internal.build.f_cpu=1000000L
attinyx5.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx5.menu.clock.128internal=128 kHz (internal)
attinyx5.menu.clock.128internal.bootloader.low_fuses=0xC4
attinyx5.menu.clock.128internal.build.f_cpu=128000L
attinyx5.menu.clock.128internal.bootloader.file=empty/empty_all.hex
attinyx5.menu.bod.disable=B.O.D. Disabled
attinyx5.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx5.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx5.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx5.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx5.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx5.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx5.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx5.build.variant=tinyX5


attinyx8.name=ATtiny48/88
attinyx8.upload.tool=avrdude
attinyx8.build.board=AVR_ATTINYX8
attinyx8.bootloader.tool=avrdude
attinyx8.bootloader.unlock_bits=0xFF
attinyx8.bootloader.lock_bits=0xFF
attinyx8.build.core=tiny
attinyx8.menu.LTO.disable=Disabled
attinyx8.menu.LTO.disable.ltocflags=
attinyx8.menu.LTO.disable.ltoelfflags=
attinyx8.menu.LTO.disable.ltocppflags=
attinyx8.menu.LTO.disable.ltoarcmd=
attinyx8.menu.LTO.enable=Enabled
attinyx8.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx8.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx8.menu.LTO.enable.ltocppflags=-flto
attinyx8.menu.LTO.enable.ltoarcmd=gcc-
attinyx8.menu.chip.88=ATtiny88
attinyx8.menu.chip.88.build.mcu=attiny88
attinyx8.menu.chip.88.upload.maximum_size=8192
attinyx8.menu.chip.88.upload.maximum_data_size=512
attinyx8.menu.chip.48=ATtiny48
attinyx8.menu.chip.48.build.mcu=attiny48
attinyx8.menu.chip.48.upload.maximum_size=4096
attinyx8.menu.chip.48.upload.maximum_data_size=256
attinyx8.bootloader.extended_fuses=0xff
attinyx8.menu.clock.8internal=8 MHz (internal)
attinyx8.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx8.menu.clock.8internal.build.f_cpu=8000000L
attinyx8.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx8.menu.clock.1internal=1 MHz (internal)
attinyx8.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx8.menu.clock.1internal.build.f_cpu=1000000L
attinyx8.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx8.menu.bod.disable=B.O.D. Disabled
attinyx8.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx8.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx8.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx8.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx8.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx8.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx8.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx8.build.variant=tinyX8


attinyx7.name=ATtiny87/167 (No bootloader)
attinyx7.upload.maximum_data_size=512
attinyx7.upload.tool=avrdude
attinyx7.build.board=AVR_ATTINYX7
attinyx7.bootloader.tool=avrdude
attinyx7.bootloader.unlock_bits=0xFF
attinyx7.bootloader.lock_bits=0xFF
attinyx7.build.core=tiny
attinyx7.bootloader.extended_fuses=0xFF
attinyx7.menu.LTO.disable=Disabled
attinyx7.menu.LTO.disable.ltocflags=
attinyx7.menu.LTO.disable.ltoelfflags=
attinyx7.menu.LTO.disable.ltocppflags=
attinyx7.menu.LTO.disable.ltoarcmd=
attinyx7.menu.LTO.enable=Enabled
attinyx7.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx7.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx7.menu.LTO.enable.ltocppflags=-flto
attinyx7.menu.LTO.enable.ltoarcmd=gcc-
attinyx7.menu.chip.167=ATtiny167
attinyx7.menu.chip.167.build.mcu=attiny167
attinyx7.menu.chip.167.upload.maximum_size=16384
attinyx7.menu.chip.87=ATtiny87
attinyx7.menu.chip.87.build.mcu=attiny87
attinyx7.menu.chip.87.upload.maximum_size=8196
attinyx7.upload.maximum_data_size=512
attinyx7.menu.clock.8internal=8 MHz (internal)
attinyx7.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx7.menu.clock.8internal.build.f_cpu=8000000L
attinyx7.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.20external=20 MHz (external)
attinyx7.menu.clock.20external.bootloader.low_fuses=0xFF
attinyx7.menu.clock.20external.build.f_cpu=20000000L
attinyx7.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.16external=16 MHz (external)
attinyx7.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx7.menu.clock.16external.build.f_cpu=16000000L
attinyx7.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.12external=12 MHz (external)
attinyx7.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx7.menu.clock.12external.build.f_cpu=12000000L
attinyx7.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.8external=8 MHz (external)
attinyx7.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx7.menu.clock.8external.build.f_cpu=8000000L
attinyx7.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.6external=6 MHz (external)
attinyx7.menu.clock.6external.bootloader.low_fuses=0xFD
attinyx7.menu.clock.6external.build.f_cpu=6000000L
attinyx7.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.4external=4 MHz (external)
attinyx7.menu.clock.4external.bootloader.low_fuses=0xFD
attinyx7.menu.clock.4external.build.f_cpu=4000000L
attinyx7.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx7.menu.clock.1internal=1 MHz (internal)
attinyx7.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx7.menu.clock.1internal.build.f_cpu=1000000L
attinyx7.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx7.menu.bod.disable=B.O.D. Disabled
attinyx7.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx7.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx7.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx7.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx7.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx7.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx7.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx7.menu.pinmapping.new=New style (down each side)
attinyx7.menu.pinmapping.new.build.variant=tinyX7_New
attinyx7.menu.pinmapping.old=Old style (SCL on 13)
attinyx7.menu.pinmapping.old.build.variant=tinyX7


attinyx7opti.name=ATtiny167/87 (Optiboot)
attinyx7opti.upload.maximum_data_size=512
attinyx7opti.upload.protocol=arduino
attinyx7opti.upload.tool=avrdude
attinyx7opti.build.board=AVR_ATTINYX7
attinyx7opti.bootloader.tool=avrdude
attinyx7opti.bootloader.unlock_bits=0xFF
attinyx7opti.bootloader.lock_bits=0xFF
attinyx7opti.build.core=tiny
attinyx7opti.bootloader.extended_fuses=0xFE
attinyx7opti.menu.LTO.disable=Disabled
attinyx7opti.menu.LTO.disable.ltocflags=
attinyx7opti.menu.LTO.disable.ltoelfflags=
attinyx7opti.menu.LTO.disable.ltocppflags=
attinyx7opti.menu.LTO.disable.ltoarcmd=
attinyx7opti.menu.LTO.enable=Enabled
attinyx7opti.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx7opti.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx7opti.menu.LTO.enable.ltocppflags=-flto
attinyx7opti.menu.LTO.enable.ltoarcmd=gcc-
attinyx7opti.menu.chip.167=ATtiny167
attinyx7opti.menu.chip.167.build.mcu=attiny167
attinyx7opti.menu.chip.167.upload.maximum_size=15744
attinyx7opti.menu.chip.87=ATtiny87
attinyx7opti.menu.chip.87.build.mcu=attiny87
attinyx7opti.menu.chip.87.upload.maximum_size=7552
attinyx7opti.bootloader.file=optiboot/optiboot_{build.mcu}_{build.f_cpu}.hex
attinyx7opti.menu.clock.8internal=8 MHz (internal)
attinyx7opti.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx7opti.menu.clock.8internal.build.f_cpu=8000000L
attinyx7opti.menu.clock.8internal.upload.speed=57600
attinyx7opti.menu.clock.16external=16 MHz (external)
attinyx7opti.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx7opti.menu.clock.16external.build.f_cpu=16000000L
attinyx7opti.menu.clock.16external.upload.speed=115200
attinyx7opti.menu.clock.12external=12 MHz (external)
attinyx7opti.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx7opti.menu.clock.12external.build.f_cpu=12000000L
attinyx7opti.menu.clock.12external.upload.speed=115200
attinyx7opti.menu.clock.8external=8 MHz (external)
attinyx7opti.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx7opti.menu.clock.8external.build.f_cpu=8000000L
attinyx7opti.menu.clock.8external.upload.speed=57600
attinyx7opti.menu.bod.disable=B.O.D. Disabled
attinyx7opti.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx7opti.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx7opti.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx7opti.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx7opti.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx7opti.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx7opti.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx7opti.menu.pinmapping.new=New style (down each side)
attinyx7opti.menu.pinmapping.new.build.variant=tinyX7_New
attinyx7opti.menu.pinmapping.old=Old style (SCL on 13)
attinyx7opti.menu.pinmapping.old.build.variant=tinyX7




attinyx61.name=ATtiny261/461/861
attinyx61.upload.maximum_size=8192
attinyx61.upload.maximum_data_size=512
attinyx61.upload.tool=avrdude
attinyx61.build.board=AVR_ATTINYX61
attinyx61.bootloader.tool=avrdude
attinyx61.bootloader.unlock_bits=0xFF
attinyx61.bootloader.lock_bits=0xFF
attinyx61.build.mcu=attiny861
attinyx61.build.core=tiny
attinyx61.menu.LTO.disable=Disabled
attinyx61.menu.LTO.disable.ltocflags=
attinyx61.menu.LTO.disable.ltoelfflags=
attinyx61.menu.LTO.disable.ltocppflags=
attinyx61.menu.LTO.disable.ltoarcmd=
attinyx61.menu.LTO.enable=Enabled
attinyx61.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx61.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx61.menu.LTO.enable.ltocppflags=-flto
attinyx61.menu.LTO.enable.ltoarcmd=gcc-
attinyx61.menu.TimerClockSource.default=CPU
attinyx61.menu.TimerClockSource.pll=64MHz
attinyx61.menu.TimerClockSource.pll.build.extra_flags=-DPLLTIMER1
attinyx61.menu.TimerClockSource.lowpll=32MHz
attinyx61.menu.TimerClockSource.lowpll.build.extra_flags=-DLOWPLLTIMER1
attinyx61.menu.chip.861=ATtiny861
attinyx61.menu.chip.861.build.mcu=attiny861
attinyx61.menu.chip.861.upload.maximum_size=8192
attinyx61.menu.chip.861.upload.maximum_data_size=512
attinyx61.menu.chip.461=ATtiny461
attinyx61.menu.chip.461.build.mcu=attiny461
attinyx61.menu.chip.461.upload.maximum_size=4096
attinyx61.menu.chip.461.upload.maximum_data_size=256
attinyx61.menu.chip.261=ATtiny261
attinyx61.menu.chip.261.build.mcu=attiny261
attinyx61.menu.chip.261.upload.maximum_size=2048
attinyx61.menu.chip.261.upload.maximum_data_size=128
attinyx61.bootloader.extended_fuses=0xFF
attinyx61.menu.clock.8internal=8 MHz (internal)
attinyx61.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx61.menu.clock.8internal.build.f_cpu=8000000L
attinyx61.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.20external=20 MHz (external)
attinyx61.menu.clock.20external.bootloader.low_fuses=0xFF
attinyx61.menu.clock.20external.build.f_cpu=20000000L
attinyx61.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.16external=16 MHz (external)
attinyx61.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx61.menu.clock.16external.build.f_cpu=16000000L
attinyx61.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.16pll=16 MHz (PLL)
attinyx61.menu.clock.16pll.bootloader.low_fuses=0xF1
attinyx61.menu.clock.16pll.build.f_cpu=16000000L
attinyx61.menu.clock.16pll.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.12external=12 MHz (external)
attinyx61.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx61.menu.clock.12external.build.f_cpu=12000000L
attinyx61.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.8external=8 MHz (external)
attinyx61.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx61.menu.clock.8external.build.f_cpu=8000000L
attinyx61.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.6external=6 MHz (external)
attinyx61.menu.clock.6external.bootloader.low_fuses=0xFD
attinyx61.menu.clock.6external.build.f_cpu=6000000L
attinyx61.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.4external=4 MHz (external)
attinyx61.menu.clock.4external.bootloader.low_fuses=0xFD
attinyx61.menu.clock.4external.build.f_cpu=4000000L
attinyx61.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx61.menu.clock.1internal=1 MHz (internal)
attinyx61.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx61.menu.clock.1internal.build.f_cpu=1000000L
attinyx61.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx61.menu.bod.disable=B.O.D. Disabled
attinyx61.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx61.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx61.menu.bod.1v8.bootloader.high_fuses=0xD6
attinyx61.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx61.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx61.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx61.menu.bod.4v3.bootloader.high_fuses=0xD4
attinyx61.build.variant=tinyX61


attinyx41.name=ATtiny441/841 (No bootloader)
attinyx41.upload.tool=avrdude
attinyx41.bootloader.tool=avrdude
attinyx41.bootloader.unlock_bits=0xFF
attinyx41.bootloader.lock_bits=0xFF
attinyx41.build.core=tinymodern
attinyx41.build.board=AVR_ATTINYX41
attinyx41.menu.chip.841=ATtiny841
attinyx41.menu.chip.841.build.mcu=attiny841
attinyx41.menu.chip.841.upload.maximum_size=8192
attinyx41.menu.chip.841.upload.maximum_data_size=512
attinyx41.menu.chip.441=ATtiny441
attinyx41.menu.chip.441.build.mcu=attiny441
attinyx41.menu.chip.441.upload.maximum_size=4096
attinyx41.menu.chip.441.upload.maximum_data_size=256
attinyx41.menu.LTO.disable=Disabled
attinyx41.menu.LTO.disable.ltocflags=
attinyx41.menu.LTO.disable.ltoelfflags=
attinyx41.menu.LTO.disable.ltocppflags=
attinyx41.menu.LTO.disable.ltoarcmd=
attinyx41.menu.LTO.enable=Enabled
attinyx41.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx41.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx41.menu.LTO.enable.ltocppflags=-flto
attinyx41.menu.LTO.enable.ltoarcmd=gcc-
attinyx41.menu.clock.8internal=8 MHz (internal)
attinyx41.menu.clock.8internal.bootloader.low_fuses=0xE2
attinyx41.menu.clock.8internal.build.f_cpu=8000000L
attinyx41.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.16external=16 MHz (external)
attinyx41.menu.clock.16external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.16external.build.f_cpu=16000000L
attinyx41.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.12external=12 MHz (external)
attinyx41.menu.clock.12external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.12external.build.f_cpu=12000000L
attinyx41.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.8external=8 MHz (external)
attinyx41.menu.clock.8external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.8external.build.f_cpu=8000000L
attinyx41.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.737external=7.372 MHz (external)
attinyx41.menu.clock.737external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.737external.build.f_cpu=7372800L
attinyx41.menu.clock.737external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.92external=9.216 MHz (external)
attinyx41.menu.clock.92external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.92external.build.f_cpu=9216000L
attinyx41.menu.clock.92external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.11external=11.0592 MHz (external)
attinyx41.menu.clock.11external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.11external.build.f_cpu=11059200L
attinyx41.menu.clock.11external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.14external=14.7456 MHz (external)
attinyx41.menu.clock.14external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.14external.build.f_cpu=14745600L
attinyx41.menu.clock.14external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.184external=18.432 MHz (external - overclocked)
attinyx41.menu.clock.184external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.184external.build.f_cpu=18432000L
attinyx41.menu.clock.184external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.1internal=1 MHz (internal)
attinyx41.menu.clock.1internal.bootloader.low_fuses=0x62
attinyx41.menu.clock.1internal.build.f_cpu=1000000L
attinyx41.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.20external=20 MHz (external - overclocked)
attinyx41.menu.clock.20external.bootloader.low_fuses=0xEE
attinyx41.menu.clock.20external.build.f_cpu=20000000L
attinyx41.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.6external=6 MHz (external)
attinyx41.menu.clock.6external.bootloader.low_fuses=0xED
attinyx41.menu.clock.6external.build.f_cpu=6000000L
attinyx41.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx41.menu.clock.4external=4 MHz (external)
attinyx41.menu.clock.4external.bootloader.low_fuses=0xED
attinyx41.menu.clock.4external.build.f_cpu=4000000L
attinyx41.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx41.menu.bod.disable=B.O.D. Disabled
attinyx41.menu.bod.disable.bootloader.extended_fuses=0xFF
attinyx41.menu.bod.disable.bootloader.high_fuses=0xD7
attinyx41.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx41.menu.bod.1v8.bootloader.extended_fuses=0xED
attinyx41.menu.bod.1v8.bootloader.high_fuses=0xD7
attinyx41.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx41.menu.bod.2v7.bootloader.extended_fuses=0xED
attinyx41.menu.bod.2v7.bootloader.high_fuses=0xD5
attinyx41.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx41.menu.bod.4v3.bootloader.extended_fuses=0xED
attinyx41.menu.bod.4v3.bootloader.high_fuses=0xD4


attiny841opti.name=ATtiny841 (Optiboot)
attiny841opti.upload.protocol=arduino
attiny841opti.upload.maximum_size=7552
attiny841opti.upload.maximum_data_size=512
attiny841opti.upload.tool=avrdude
attiny841opti.bootloader.tool=avrdude
attiny841opti.bootloader.unlock_bits=0xFF
attiny841opti.bootloader.lock_bits=0xFF
attiny841opti.build.mcu=attiny841
attiny841opti.build.core=tinymodern
attiny841opti.build.board=AVR_ATTINY841_OPTIBOOT
attiny841opti.bootloader.extended_fuses=0xFE
attiny841opti.bootloader.high_fuses=0xD7
attiny841opti.menu.LTO.disable=Disabled
attiny841opti.menu.LTO.disable.ltocflags=
attiny841opti.menu.LTO.disable.ltoelfflags=
attiny841opti.menu.LTO.disable.ltocppflags=
attiny841opti.menu.LTO.disable.ltoarcmd=
attiny841opti.menu.LTO.enable=Enabled
attiny841opti.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attiny841opti.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attiny841opti.menu.LTO.enable.ltocppflags=-flto
attiny841opti.menu.LTO.enable.ltoarcmd=gcc-
attiny841opti.menu.clock.8internal=8 MHz (internal)
attiny841opti.menu.clock.8internal.bootloader.low_fuses=0xE2
attiny841opti.menu.clock.8internal.build.f_cpu=8000000L
attiny841opti.menu.clock.8internal.bootloader.file=optiboot/optiboot_attiny841at8.hex
attiny841opti.menu.clock.8internal.upload.speed=57600
attiny841opti.menu.clock.16external=16 MHz (external)
attiny841opti.menu.clock.16external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.16external.build.f_cpu=16000000L
attiny841opti.menu.clock.16external.bootloader.file=optiboot/optiboot_attiny841at16.hex
attiny841opti.menu.clock.16external.upload.speed=115200
attiny841opti.menu.clock.12external=12 MHz (external)
attiny841opti.menu.clock.12external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.12external.build.f_cpu=12000000L
attiny841opti.menu.clock.12external.bootloader.file=optiboot/optiboot_attiny841at12.hex
attiny841opti.menu.clock.12external.upload.speed=115200
attiny841opti.menu.clock.8external=8 MHz (external)
attiny841opti.menu.clock.8external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.8external.build.f_cpu=8000000L
attiny841opti.menu.clock.8external.bootloader.file=optiboot/optiboot_attiny841at8.hex
attiny841opti.menu.clock.8external.upload.speed=57600
attiny841opti.menu.clock.8internal5v=8 MHz (internal, Vcc > 4v)
attiny841opti.menu.clock.8internal5v.bootloader.low_fuses=0xE2
attiny841opti.menu.clock.8internal5v.build.f_cpu=8200000L
attiny841opti.menu.clock.8internal5v.bootloader.file=optiboot/optiboot_attiny841at8_5v.hex
attiny841opti.menu.clock.8internal5v.upload.speed=57600
attiny841opti.menu.clock.737external=7.3728 MHz (external)
attiny841opti.menu.clock.737external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.737external.build.f_cpu=7372800L
attiny841opti.menu.clock.737external.bootloader.file=optiboot/optiboot_attiny841at732.hex
attiny841opti.menu.clock.737external.upload.speed=57600
attiny841opti.menu.clock.921external=9.216 MHz (external)
attiny841opti.menu.clock.921external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.921external.build.f_cpu=9216000L
attiny841opti.menu.clock.921external.bootloader.file=optiboot/optiboot_attiny841at921.hex
attiny841opti.menu.clock.921external.upload.speed=57600
attiny841opti.menu.clock.110external=11.0592 MHz (external)
attiny841opti.menu.clock.110external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.110external.build.f_cpu=11059200L
attiny841opti.menu.clock.110external.bootloader.file=optiboot/optiboot_attiny841at110.hex
attiny841opti.menu.clock.110external.upload.speed=115200
attiny841opti.menu.clock.147external=14.7456 MHz (external)
attiny841opti.menu.clock.147external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.147external.build.f_cpu=14745600L
attiny841opti.menu.clock.147external.bootloader.file=optiboot/optiboot_attiny841at147.hex
attiny841opti.menu.clock.147external.upload.speed=115200
attiny841opti.menu.clock.184external=18.432 MHz (external - overclocked)
attiny841opti.menu.clock.184external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.184external.build.f_cpu=18432000L
attiny841opti.menu.clock.184external.bootloader.file=optiboot/optiboot_attiny841at184.hex
attiny841opti.menu.clock.184external.upload.speed=115200
attiny841opti.menu.clock.20external=20 MHz (external - overclocked)
attiny841opti.menu.clock.20external.bootloader.low_fuses=0xEE
attiny841opti.menu.clock.20external.build.f_cpu=20000000L
attiny841opti.menu.clock.20external.bootloader.file=optiboot/optiboot_attiny841at20.hex
attiny841opti.menu.clock.20external.upload.speed=115200
attiny841opti.menu.bod.disable=B.O.D. Disabled
attiny841opti.menu.bod.disable.bootloader.extended_fuses=0xFE
attiny841opti.menu.bod.disable.bootloader.high_fuses=0xD7
attiny841opti.menu.bod.1v8=B.O.D. Enabled (1.8v)
attiny841opti.menu.bod.1v8.bootloader.extended_fuses=0xEC
attiny841opti.menu.bod.1v8.bootloader.high_fuses=0xD7
attiny841opti.menu.bod.2v7=B.O.D. Enabled (2.7v)
attiny841opti.menu.bod.2v7.bootloader.extended_fuses=0xEC
attiny841opti.menu.bod.2v7.bootloader.high_fuses=0xD5
attiny841opti.menu.bod.4v3=B.O.D. Enabled (4.3v)
attiny841opti.menu.bod.4v3.bootloader.extended_fuses=0xEC
attiny841opti.menu.bod.4v3.bootloader.high_fuses=0xD4


attiny828.name=ATtiny828 (No bootloader)
attiny828.upload.maximum_size=8192
attiny828.upload.maximum_data_size=512
attiny828.upload.tool=avrdude
attiny828.bootloader.tool=avrdude
attiny828.bootloader.unlock_bits=0x3F
attiny828.bootloader.lock_bits=0x3F
attiny828.build.mcu=attiny828
attiny828.build.core=tinymodern
attiny828.build.board=AVR_ATTINY828
attiny828.menu.LTO.disable=Disabled
attiny828.menu.LTO.disable.ltocflags=
attiny828.menu.LTO.disable.ltoelfflags=
attiny828.menu.LTO.disable.ltocppflags=
attiny828.menu.LTO.disable.ltoarcmd=
attiny828.menu.LTO.enable=Enabled
attiny828.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attiny828.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attiny828.menu.LTO.enable.ltocppflags=-flto
attiny828.menu.LTO.enable.ltoarcmd=gcc-
attiny828.menu.clock.8internal=8 MHz (internal)
attiny828.menu.clock.8internal.bootloader.low_fuses=0xEE
attiny828.menu.clock.8internal.build.f_cpu=8000000L
attiny828.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attiny828.menu.clock.1internal=1 MHz (internal)
attiny828.menu.clock.1internal.bootloader.low_fuses=0x6E
attiny828.menu.clock.1internal.build.f_cpu=1000000L
attiny828.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attiny828.menu.bod.disable=Disabled
attiny828.menu.bod.disable.bootloader.extended_fuses=0xFF
attiny828.menu.bod.disable.bootloader.high_fuses=0xD7
attiny828.menu.bod.1v8=B.O.D. Enabled (1.8v)
attiny828.menu.bod.1v8.bootloader.extended_fuses=0x5F
attiny828.menu.bod.1v8.bootloader.high_fuses=0xD7
attiny828.menu.bod.2v7=B.O.D. Enabled (2.7v)
attiny828.menu.bod.2v7.bootloader.extended_fuses=0x5F
attiny828.menu.bod.2v7.bootloader.high_fuses=0xD5
attiny828.menu.bod.4v3=B.O.D. Enabled (4.3v)
attiny828.menu.bod.4v3.bootloader.extended_fuses=0x5F
attiny828.menu.bod.4v3.bootloader.high_fuses=0xD4


attiny828opti.name=ATtiny828 (Optiboot)
attiny828opti.upload.maximum_size=7680
attiny828opti.upload.maximum_data_size=512
attiny828opti.upload.protocol=arduino
attiny828opti.upload.speed=57600
attiny828opti.upload.tool=avrdude
attiny828opti.bootloader.tool=avrdude
attiny828opti.bootloader.unlock_bits=0x3F
attiny828opti.bootloader.lock_bits=0x3F
attiny828opti.build.mcu=attiny828
attiny828opti.build.core=tinymodern
attiny828opti.build.board=AVR_ATTINY828
attiny828opti.bootloader.low_fuses=0xEE
attiny828opti.menu.LTO.disable=Disabled
attiny828opti.menu.LTO.disable.ltocflags=
attiny828opti.menu.LTO.disable.ltoelfflags=
attiny828opti.menu.LTO.disable.ltocppflags=
attiny828opti.menu.LTO.disable.ltoarcmd=
attiny828opti.menu.LTO.enable=Enabled
attiny828opti.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attiny828opti.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attiny828opti.menu.LTO.enable.ltocppflags=-flto
attiny828opti.menu.LTO.enable.ltoarcmd=gcc-
attiny828opti.menu.vcc.3v3=Under 4.0 V
attiny828opti.menu.vcc.3v3.build.f_cpu=8000000L
attiny828opti.menu.vcc.3v3.bootloader.file=optiboot/optiboot_attiny828at8.hex
attiny828opti.menu.vcc.5v=Over 4.0 V
attiny828opti.menu.vcc.5v.build.f_cpu=8200000L
attiny828opti.menu.vcc.5v.bootloader.file=optiboot/optiboot_attiny828at8_5v.hex
attiny828opti.menu.bod.disable=Disabled
attiny828opti.menu.bod.disable.bootloader.extended_fuses=0xFA
attiny828opti.menu.bod.disable.bootloader.high_fuses=0xD7
attiny828opti.menu.bod.1v8=B.O.D. Enabled (1.8v)
attiny828opti.menu.bod.1v8.bootloader.extended_fuses=0x5A
attiny828opti.menu.bod.1v8.bootloader.high_fuses=0xD7
attiny828opti.menu.bod.2v7=B.O.D. Enabled (2.7v)
attiny828opti.menu.bod.2v7.bootloader.extended_fuses=0x5A
attiny828opti.menu.bod.2v7.bootloader.high_fuses=0xD5
attiny828opti.menu.bod.4v3=B.O.D. Enabled (4.3v)
attiny828opti.menu.bod.4v3.bootloader.extended_fuses=0x5A
attiny828opti.menu.bod.4v3.bootloader.high_fuses=0xD4


attiny1634.name=ATtiny1634 (No bootloader)
attiny1634.upload.maximum_size=16384
attiny1634.upload.maximum_data_size=1024
attiny1634.upload.tool=avrdude
attiny1634.bootloader.tool=avrdude
attiny1634.bootloader.unlock_bits=0xFF
attiny1634.bootloader.lock_bits=0xFF
attiny1634.build.mcu=attiny1634
attiny1634.build.core=tinymodern
attiny1634.build.board=AVR_ATTINY1634
attiny1634.bootloader.extended_fuses=0xFF
attiny1634.bootloader.high_fuses=0xD7
attiny1634.menu.LTO.disable=Disabled
attiny1634.menu.LTO.disable.ltocflags=
attiny1634.menu.LTO.disable.ltoelfflags=
attiny1634.menu.LTO.disable.ltocppflags=
attiny1634.menu.LTO.disable.ltoarcmd=
attiny1634.menu.LTO.enable=Enabled
attiny1634.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attiny1634.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attiny1634.menu.LTO.enable.ltocppflags=-flto
attiny1634.menu.LTO.enable.ltoarcmd=gcc-
attiny1634.menu.clock.8internal=8 MHz (internal)
attiny1634.menu.clock.8internal.bootloader.low_fuses=0xE2
attiny1634.menu.clock.8internal.build.f_cpu=8000000L
attiny1634.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.12external=12 MHz (external)
attiny1634.menu.clock.12external.bootloader.low_fuses=0xEF
attiny1634.menu.clock.12external.build.f_cpu=12000000L
attiny1634.menu.clock.12external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.8external=8 MHz (external)
attiny1634.menu.clock.8external.bootloader.low_fuses=0xEF
attiny1634.menu.clock.8external.build.f_cpu=8000000L
attiny1634.menu.clock.8external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.737external=7.372 MHz (external)
attiny1634.menu.clock.737external.bootloader.low_fuses=0xEE
attiny1634.menu.clock.737external.build.f_cpu=7372800L
attiny1634.menu.clock.737external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.92external=9.216 MHz (external)
attiny1634.menu.clock.92external.bootloader.low_fuses=0xEE
attiny1634.menu.clock.92external.build.f_cpu=9216000L
attiny1634.menu.clock.92external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.11external=11.0592 MHz (external)
attiny1634.menu.clock.11external.bootloader.low_fuses=0xEE
attiny1634.menu.clock.11external.build.f_cpu=11059200L
attiny1634.menu.clock.11external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.143external=14.7456 MHz (external - overclocked)
attiny1634.menu.clock.143external.bootloader.low_fuses=0xEE
attiny1634.menu.clock.143external.build.f_cpu=14745600L
attiny1634.menu.clock.143external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.6external=6 MHz (external)
attiny1634.menu.clock.6external.bootloader.low_fuses=0xEF
attiny1634.menu.clock.6external.build.f_cpu=6000000L
attiny1634.menu.clock.6external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.4external=4 MHz (external)
attiny1634.menu.clock.4external.bootloader.low_fuses=0xEF
attiny1634.menu.clock.4external.build.f_cpu=6000000L
attiny1634.menu.clock.4external.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.1internal=1 MHz (internal)
attiny1634.menu.clock.1internal.bootloader.low_fuses=0x62
attiny1634.menu.clock.1internal.build.f_cpu=1000000L
attiny1634.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attiny1634.menu.clock.16external=16 MHz (external - overclocked)
attiny1634.menu.clock.16external.bootloader.low_fuses=0xEF
attiny1634.menu.clock.16external.build.f_cpu=16000000L
attiny1634.menu.clock.16external.bootloader.file=empty/empty_all.hex
attiny1634.menu.bod.disable=Disabled
attiny1634.menu.bod.disable.bootloader.extended_fuses=0xFF
attiny1634.menu.bod.disable.bootloader.high_fuses=0xD7
attiny1634.menu.bod.1v8=B.O.D. Enabled (1.8v)
attiny1634.menu.bod.1v8.bootloader.extended_fuses=0xFD
attiny1634.menu.bod.1v8.bootloader.high_fuses=0xD7
attiny1634.menu.bod.2v7=B.O.D. Enabled (2.7v)
attiny1634.menu.bod.2v7.bootloader.extended_fuses=0xFD
attiny1634.menu.bod.2v7.bootloader.high_fuses=0xD5
attiny1634.menu.bod.4v3=B.O.D. Enabled (4.3v)
attiny1634.menu.bod.4v3.bootloader.extended_fuses=0xFD
attiny1634.menu.bod.4v3.bootloader.high_fuses=0xD4

attiny1634opti.name=ATtiny1634 (Optiboot)
attiny1634opti.upload.maximum_size=15744
attiny1634opti.upload.maximum_data_size=1024
attiny1634opti.upload.protocol=arduino
attiny1634opti.upload.tool=avrdude
attiny1634opti.bootloader.tool=avrdude
attiny1634opti.bootloader.unlock_bits=0xFF
attiny1634opti.bootloader.lock_bits=0xFF
attiny1634opti.build.mcu=attiny1634
attiny1634opti.build.core=tinymodern
attiny1634opti.build.board=AVR_ATTINY1634_OPTIBOOT
attiny1634opti.bootloader.extended_fuses=0xFE
attiny1634opti.bootloader.high_fuses=0xD7
attiny1634opti.menu.LTO.disable=Disabled
attiny1634opti.menu.LTO.disable.ltocflags=
attiny1634opti.menu.LTO.disable.ltoelfflags=
attiny1634opti.menu.LTO.disable.ltocppflags=
attiny1634opti.menu.LTO.disable.ltoarcmd=
attiny1634opti.menu.LTO.enable=Enabled
attiny1634opti.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attiny1634opti.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attiny1634opti.menu.LTO.enable.ltocppflags=-flto
attiny1634opti.menu.LTO.enable.ltoarcmd=gcc-
attiny1634opti.menu.clock.8internal=8 MHz (internal)
attiny1634opti.menu.clock.8internal.bootloader.low_fuses=0xE2
attiny1634opti.menu.clock.8internal.build.f_cpu=8000000L
attiny1634opti.menu.clock.8internal.bootloader.file=optiboot/optiboot_attiny1634at8.hex
attiny1634opti.menu.clock.8internal.upload.speed=57600
attiny1634opti.menu.clock.12external=12 MHz (external)
attiny1634opti.menu.clock.12external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.12external.build.f_cpu=12000000L
attiny1634opti.menu.clock.12external.bootloader.file=optiboot/optiboot_attiny1634at12.hex
attiny1634opti.menu.clock.12external.upload.speed=115200
attiny1634opti.menu.clock.8external=8 MHz (external)
attiny1634opti.menu.clock.8external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.8external.build.f_cpu=8000000L
attiny1634opti.menu.clock.8external.bootloader.file=optiboot/optiboot_attiny1634at8.hex
attiny1634opti.menu.clock.8external.upload.speed=57600
attiny1634opti.menu.clock.8internal5v=8 MHz (internal, Vcc > 4v)
attiny1634opti.menu.clock.8internal5v.bootloader.low_fuses=0xE2
attiny1634opti.menu.clock.8internal5v.build.f_cpu=8200000L
attiny1634opti.menu.clock.8internal5v.bootloader.file=optiboot/optiboot_attiny1634at8_5v.hex
attiny1634opti.menu.clock.8internal5v.upload.speed=57600
attiny1634opti.menu.clock.737external=7.3728 MHz (external)
attiny1634opti.menu.clock.737external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.737external.build.f_cpu=7372800L
attiny1634opti.menu.clock.737external.bootloader.file=optiboot/optiboot_attiny1634at737.hex
attiny1634opti.menu.clock.737external.upload.speed=57600
attiny1634opti.menu.clock.921external=9.216 MHz (external)
attiny1634opti.menu.clock.921external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.921external.build.f_cpu=9216000L
attiny1634opti.menu.clock.921external.bootloader.file=optiboot/optiboot_attiny1634at921.hex
attiny1634opti.menu.clock.921external.upload.speed=57600
attiny1634opti.menu.clock.110external=11.059 MHz (external)
attiny1634opti.menu.clock.110external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.110external.build.f_cpu=11059200L
attiny1634opti.menu.clock.110external.bootloader.file=optiboot/optiboot_attiny1634at110.hex
attiny1634opti.menu.clock.110external.upload.speed=115200
attiny1634opti.menu.clock.147external=14.7456 MHz (external - overclocked)
attiny1634opti.menu.clock.147external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.147external.build.f_cpu=14745600L
attiny1634opti.menu.clock.147external.bootloader.file=optiboot/optiboot_attiny1634at147.hex
attiny1634opti.menu.clock.147external.upload.speed=115200
attiny1634opti.menu.clock.16external=16 MHz (external - overclocked)
attiny1634opti.menu.clock.16external.bootloader.low_fuses=0xEF
attiny1634opti.menu.clock.16external.build.f_cpu=16000000L
attiny1634opti.menu.clock.16external.bootloader.file=optiboot/optiboot_attiny1634at16.hex
attiny1634opti.menu.clock.16external.upload.speed=115200
attiny1634opti.menu.bod.disable=B.O.D. Disabled
attiny1634opti.menu.bod.disable.bootloader.extended_fuses=0xFE
attiny1634opti.menu.bod.disable.bootloader.high_fuses=0xD7
attiny1634opti.menu.bod.1v8=B.O.D. Enabled (1.8v)
attiny1634opti.menu.bod.1v8.bootloader.extended_fuses=0xFC
attiny1634opti.menu.bod.1v8.bootloader.high_fuses=0xD7
attiny1634opti.menu.bod.2v7=B.O.D. Enabled (2.7v)
attiny1634opti.menu.bod.2v7.bootloader.extended_fuses=0xFC
attiny1634opti.menu.bod.2v7.bootloader.high_fuses=0xD5
attiny1634opti.menu.bod.4v3=B.O.D. Enabled (4.3v)
attiny1634opti.menu.bod.4v3.bootloader.extended_fuses=0xFC
attiny1634opti.menu.bod.4v3.bootloader.high_fuses=0xD4


attinyx313.name=ATtiny2313/4313
attinyx313.upload.maximum_size=4096
attinyx313.upload.maximum_data_size=256
attinyx313.upload.tool=avrdude
attinyx313.bootloader.tool=avrdude
attinyx313.bootloader.unlock_bits=0xFF
attinyx313.bootloader.lock_bits=0xFF
attinyx313.build.core=tiny
attinyx313.build.board=AVR_ATTINYX313
attinyx313.bootloader.extended_fuses=0xFF
attinyx313.menu.LTO.disable=Disabled
attinyx313.menu.LTO.disable.ltocflags=
attinyx313.menu.LTO.disable.ltoelfflags=
attinyx313.menu.LTO.disable.ltocppflags=
attinyx313.menu.LTO.disable.ltoarcmd=
attinyx313.menu.LTO.enable=Enabled
attinyx313.menu.LTO.enable.ltocflags=-flto -fno-fat-lto-objects
attinyx313.menu.LTO.enable.ltoelfflags=-flto -fuse-linker-plugin
attinyx313.menu.LTO.enable.ltocppflags=-flto
attinyx313.menu.LTO.enable.ltoarcmd=gcc-
attinyx313.menu.chip.4313=ATtiny4313
attinyx313.menu.chip.4313.build.mcu=attiny4313
attinyx313.menu.chip.4313.upload.maximum_size=4096
attinyx313.menu.chip.4313.upload.maximum_data_size=256
attinyx313.menu.chip.2313=ATtiny2313
attinyx313.menu.chip.2313.build.mcu=attiny2313
attinyx313.menu.chip.2313.upload.maximum_size=2048
attinyx313.menu.chip.2313.upload.maximum_data_size=128
attinyx313.menu.clock.8internal=8 MHz (internal)
attinyx313.menu.clock.8internal.bootloader.low_fuses=0xE4
attinyx313.menu.clock.8internal.build.f_cpu=8000000L
attinyx313.menu.clock.8internal.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.20external=20 MHz (external)
attinyx313.menu.clock.20external.bootloader.low_fuses=0xFF
attinyx313.menu.clock.20external.build.f_cpu=20000000L
attinyx313.menu.clock.20external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.16external=16 MHz (external)
attinyx313.menu.clock.16external.bootloader.low_fuses=0xFF
attinyx313.menu.clock.16external.build.f_cpu=16000000L
attinyx313.menu.clock.16external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.12external=12 MHz (external)
attinyx313.menu.clock.12external.bootloader.low_fuses=0xFF
attinyx313.menu.clock.12external.build.f_cpu=12000000L
attinyx313.menu.clock.12external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.8external=8 MHz (external)
attinyx313.menu.clock.8external.bootloader.low_fuses=0xFF
attinyx313.menu.clock.8external.build.f_cpu=8000000L
attinyx313.menu.clock.8external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.1internal=1 MHz (internal)
attinyx313.menu.clock.1internal.bootloader.low_fuses=0x64
attinyx313.menu.clock.1internal.build.f_cpu=1000000L
attinyx313.menu.clock.1internal.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.4internal=4 MHz (internal)
attinyx313.menu.clock.4internal.bootloader.low_fuses=0xE2
attinyx313.menu.clock.4internal.build.f_cpu=4000000L
attinyx313.menu.clock.4internal.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.6external=6 MHz (external)
attinyx313.menu.clock.6external.bootloader.low_fuses=0xFD
attinyx313.menu.clock.6external.build.f_cpu=6000000L
attinyx313.menu.clock.6external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.4external=4 MHz (external)
attinyx313.menu.clock.4external.bootloader.low_fuses=0xFD
attinyx313.menu.clock.4external.build.f_cpu=4000000L
attinyx313.menu.clock.4external.bootloader.file=empty/empty_all.hex
attinyx313.menu.clock.5internal=0.5 MHz (internal)
attinyx313.menu.clock.5internal.bootloader.low_fuses=0x62
attinyx313.menu.clock.5internal.build.f_cpu=500000L
attinyx313.menu.clock.5internal.bootloader.file=empty/empty_all.hex
attinyx313.menu.bod.disable=B.O.D. Disabled
attinyx313.menu.bod.disable.bootloader.high_fuses=0x9F
attinyx313.menu.bod.1v8=B.O.D. Enabled (1.8v)
attinyx313.menu.bod.1v8.bootloader.high_fuses=0x9D
attinyx313.menu.bod.2v7=B.O.D. Enabled (2.7v)
attinyx313.menu.bod.2v7.bootloader.high_fuses=0x9B
attinyx313.menu.bod.4v3=B.O.D. Enabled (4.3v)
attinyx313.menu.bod.4v3.bootloader.high_fuses=0x99
attinyx313.menu.INITIALIZE_SECONDARY_TIMERS.0=no
attinyx313.menu.INITIALIZE_SECONDARY_TIMERS.1=yes
attinyx313.menu.INITIALIZE_SECONDARY_TIMERS.1.build.extra_flags=-DINITIALIZE_SECONDARY_TIMERS=1
attinyx313.build.variant=tinyX313

